fbeat = |f1 –f2|

fn =nf1 open-end pipe or standing wave

fn =(2n – 1)f1 closed end pipe

vmax = ὠA

amax = ὠA

f = $\frac{v}{4L}$ fundamental frequency for a closed pipe